Commander Wi-Fi access (Vijeo Air app)
Version date: 7/5/2018
Warning
You must consider the potential of accidental touches from remote mobile devices.  Know and understand the hazards regarding equipment movement started by a remote operation.   You, as the operator, are responsible for all gates and interlock for protecting people and equipment.

Failure to follow these instructions can result in death, serious injury, or equipment damage.

Required Hardware (source locally)
	Wi-Fi router
	Ethernet cable
	Tablet or cell phone with Wi-Fi capability

Hardware installation
Locate Wi-Fi router in a suitable location near the HMI enclosure.
The Wi-Fi router should be powered by its own power supply.
Connect an ethernet cable from Wi-Fi router to the ethernet switch inside the HMI enclosure. 

Router configuration
	Configure router 
static IP address 	10.10.11.5
subnet mask 		255.255.255.0
gateway 		10.10.11.211
	Set router name (NECO dryer).
Set router security password to prevent unauthorized access.
	
Record security password here _______________________________________

Required Software (download app)
	Schneider Vijeo Design’Air (available on google apps)
	
Tablet / Phone Wi-Fi settings
	Connect to router (NECO dryer).
Enter router security password.




Initial Vijeo Design’Air app settings
	Press		“+ Add device” icon
	Name: 		NECO dryer
	Host:		10.10.11.101
	Port:		37891
	Press 		“OK”
Using the Vijeo Air app
Note:  The use of this app allows remote access to monitor, make minor operational setting changes and to stop the dryer only.  Starting of equipment must be performed at the dryer HMI panel.

The local operator (User, Owner or NecoTech) via the HMI must start and get the dryer and associated equipment in the desire state of operation.

Once all equipment is running as desired, the local operator enables remote access
MAIN MENU > SETUP > SECURITY SETUP > I ACCEPT > ENABLE REMOTE ACCESS.

When the “ENABLE REMOTE ACCESS” icon is pressed the current operator is logged out and the “Remote” user is logged in on the HMI.

The user is now able to access the dryer control via the Vijeo Design’Air app.
Press the app icon on the tablet / phone, then press “NECO dryer”.

Read accept the liability statement.  Press “OK” or “View-only” icon.
Login.  
Username:	RemoteWiFi
Password:	1379
Press		“OK”

At this point the tablet / phone displays the same image the HMI screen.
The operator may remotely
change Burner Temperature(s)
change Target Moisture
[bookmark: _GoBack]change Manual Metering Speed Setpoint
and view all screens

Note: If the “LOGOUT” icon is pressed the dryer control will not be able accessible until operator locally re-enables the remote access.

