PLC Firmware loading
Turn off power—1CB
Insert the SD card
Turn power back on—1CB
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Description automatically generated]SD Light is on for Approx. 2+ minutes
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Description automatically generated]ERR light comes on, loading is finished.
Turn power off 1CB, remove SD card

Turn Power back on 1CB
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   The initial lights
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Description automatically generated with medium confidence]

Then just then err light is on.
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Description automatically generated]

When the ETN (ethernet) light comes on and the err light blinks the PLC is ready for a program.
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